f NOTES:
	1-		Date Code located on bottom of handle.
	7-		Static protection to be used when handling.
	18-		Torque to 13-18 in./lbs.
	29-		Torque to 140-160 in./lbs.-Nosepiece to bearing retainer.

LUBRICATION:
Lubricate clutches & spindles with approximately .5 grams (1/6 oz.) of clutch grease.

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.