NOTES:

4,22,38  Install negator (spring) assembly (ITEM 4) into the back of the pusher (ITEM 22).  The clip on the end of the spring should be towards the left side of the magazine.  Install the hub/pusher into the back of magazine and slide all the way forward while keeping the magazine pointed down.  While keeping the magazine level, reach into the front with a piece of stiff wire bent at 90 degrees to engage the clip on the end of the spring.  Pull clip out and engage on the side of the magazine.  
21	 	    After inserting into magazine, bend the two tabs back on the left and right side to keep in place.    	  
30        Torque to 150-170 in-lbs.
38  Any magazine repair/replacement on any framing tool that has a date code of 200417 or earlier MUST have the upper contact trip replaced using part number 617170-00 if the new replacement magazine does not have the key hole slot.  See SB06063 for details.   
48	To remove, first remove ITEM 3.
57			Torque to 190-205 in-lbs.
58,63 	Torque to 35-45 in-lbs.
59,60	Torque to 20-30 in-lbs.
62			Torque to 80-95 in-lbs.
67			Torque to 55-65 in-lbs.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.